

// Parameter

Open the PSF with Neill Corlett's "PSF-o-Cycle" application to adjust
the following parameters.


NAME				INFORMATION
-------------------------------------------
SEQ/SEP/VAG Address		Location of SEQ, SEP or VAG data. You
				may select any location you wish, but
				it must be 0x80040000 or higher.

				Default is 0x800A0000

VH Address			Location of VH data. This is ignored
				when using VAG data.

				Default is 0x800E0000

VB Address			Location of VB data. This is ignored
				when using VAG data.

				Default is 0x80160000

Playback Type			0=SEP, 1=SEQ, 2=VAG
				By default, this parameter is set to
				1 for SEQ data.

Playback Amount			0=SSPLAY_INFINITY, Non-Zero=SSPLAY_PLAY
				By default, this parameter is set to
				0 for infinite playback looping.

Automatic Stop			0=OFF, 1=ON
				When active, playback will automatically
				stop when the end of sequence playback
				is reached.

SEP Play Mode			0 = Only Play Sequence ID #1
				1 = Play Sequence ID #2 after Sequence ID #1
				2 = Play both Sequence ID #1 and #2 at once
				This option is available for SEP archive
				files, only.

Sequence Amount			Must be set to 1 for SEQ data, otherwise, the
				amount of SEQ contained within a SEP file.

Sequence ID #1			Must be 0 for SEQ data.

Sequence ID #2			SEP use, only - ignored with SEQ data.

Sequence Tick Mode		0=NONE (DO NOT USE)
				1=1/60 second (NTSC)
				2=1/240 second
				3=1/120 second
				4=1/50 second (PAL)
				5=VSYNC (NTSC/PAL)
				6=MAX
				By default, this parameter is set to
				1/60 second (NTSC).

Reverb Mode			0=OFF
				1=ROOM
				2=STUDIOA
				3=STUDIOB
				4=STUDIOC
				5=HALL
				6=SPACE
				7=ECHO
				8=DELAY
				9=PIPE
				10=MAX
				By default, this parameter is set to
				OFF.

Reverb Depth (L/R)		Active only when Reverb Mode is not OFF.

Reverb Delay			Active only when Reverb Mode is not OFF
				and when the Mode is either ECHO or DELAY.

Reverb Feedback			Active only when Reverb Mode is not OFF
				and when the Mode is DELAY.

Reverb Volume (L/R)		Active only when Reverb Mode is not OFF.

Master Volume (L/R)		127 by default

Sequence Volume (L/R)		110 by default

VAB ID				Unused, for now - leave it set to 0.

VAB Transfer Mode		Unused, for now - leave it set to 0.

VAB Non-Zero Volume		0=OFF, 1=ON
				When active, this option will correct any
				VAB data with volume set to zero (0).
				This feature is useful for tracks that
				are properly created but don't seem to
				playback (Resident Evil 2 SFX, for example).

VAB High-Priority		0=OFF, 1=ON
				When active, all VAB program Modes become
				a high-priority. PSF plugins disregard this,
				so it's affect is useless, here.

Video Mode			0=NTSC, 1=PAL
				Useful for nostalgia purpose, only (when
				used with VSYNC Sequence Tick Mode).

Channel Output			0=Stereo, 1=Mono
				PSF plugins disregard this, so it's affect
				is useless, here.

Custom Tempo?			0=OFF, 1=ON
Custom Tempo Value		Used with 'Custom Tempo?'

Custom Accelerando?		0=OFF, 1=ON
Custom Crescendo?		0=OFF, 1=ON
Custom Decrescendo?		0=OFF, 1=ON
Custom Ritardando?		0=OFF, 1=ON
Custom Tick Skip?		0=OFF, 1=ON
Custom Tick Resolution		Used with Custom settings
Custom Tick Skip Unit		Used with Custom settings
Custom Tick Skip Value		Used with Custom settings
Custom Tick Timing		Used with Custom settings
De/Crescendo Volume		Used with Custom settings

Mute Channel X			0=OFF, 1=ON
				When active, the corresponding MIDI channel
				will be muted during all playback.
